LOCKERS
(15-41000, 15-42000, 15-43000, 15-44000)

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Extra Wide Heavy Duty Plastic Lockers.

1.2	REFERENCES

A.	IBC - International Building Code.
B.	LEED Submittal Requirements NC v3.0:  Sustainable Design Requirements – LEED for New Construction and the LEED NC v3.0 reference guide.
C.	GREENGUARD Environmental Institute (GREENGUARD):
1.  GREENGUARD certified low emitting products.

1.3	RELATED SECTIONS
A.	Section 03300 (03 30 00) – Cast-in-Place Concrete:  Concrete bases.
B.	Section 06100 (06 10 00) – Rough Carpentry:  Wood ground and furring for anchoring lockers.
C.	Section 09650 (09 65 13.13) – Resilient Base.

1.4	SUBMITTALS
A.	Submit under provisions of Section 013300.
B.	Product Data:  Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
C.	Shop Drawings:  Prepared specifically for this project; show dimensions of lockers and interface with other products.
D.	Submit under provisions of LEED NC v3.0 reference guide:  Product data for each type of accessory specified, with installation instructions for each unit built-in or connected to other construction:
1.	Product Data for Credit MR 4 – Recycled Content:  For products having recycled content, documentation indicating percentages by weight of post-consumer and pre-consumer recycled content.
2.	Product Data for Credit MR 5 – Regional Materials:  Provide documentation indicating where materials have been extracted, harvested or recovered, as well as manufactured.  If only a portion of the product has been extracted, harvested or recovered, and manufactured within 500 miles of the job site, then indicate that percentage.
3.	Product Data for IEQ 4.1 – Low Emitting Materials-Adhesives and Sealants:  Provide documentation including printed statement of VOC content for all adhesives and sealants.
4.	Laboratory Test Reports for Credit IEQ 4.2:  For primers, documentation indicating that products comply with the testing and product requirements of the California Department of Health Services’ “Standard Practice for the Testing of Volatile Organic Emissions from Various Sources Using Small-Scale Environmental Chambers”.
5.	Indoor Environmental Quality Certification:  Provide certificate indicated that products have been certified under the following programs, or a comparable certification acceptable to Owner:
	a.	GREENGUARD Indoor Air Quality Certified.
	b.	GREENGUARD Certified for Children and Schools.
E.	Selection Samples:  For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and patterns.

1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications:  Manufacturer shall have a Quality System in place to ensure and be able to substantiate that manufactured units conform to requirements and match the approved design and must be ISO 9001:2015 certified.

1.6	DELIVERY, STORAGE, AND HANDLING
A.	Store products in manufacturer's unopened packaging until ready for installation.
B.	Locker components shall be shipped fully assembled. All finishes shall be protected from soiling and damage during handling.
C.	Store and dispose of solvent-based materials, and materials used with solvent-based materials, in accordance with requirements of local authorities having jurisdiction.
D.	Do not deliver plastic lockers to the site until the building is enclosed and HVAC systems are in operation.  Deliver plastic lockers in manufacturer's original packaging.  Store in an upright condition. Protect plastic lockers from exposure to direct sunlight.

1.7	WARRANTY
A.	Manufacturer's standard warranty to repair or replace components of locker products that fail in materials or workmanship within 3 years from date of Substantial Completion.

PART 2    PRODUCTS
2.1	LOCKERS
Single-tier, double-tier, triple-tier and four-tier extra wide heavy duty plastic lockers:  Constructed of water resistant 1/2 inch (12.7 mm) thick high density polyethylene (HDPE); includes stainless steel hinges and a stainless steel hasp for locking; can accommodate combination padlocks or key padlocks.

A.	Extra Wide Heavy Duty Plastic Locker Series:
1.	15-41000 series:  Single-tier.
2.	15-42000 series:  Double-tier.
3.	15-43000 series:  Triple-tier.
4.	15-44000 series:  Four-tier.

B.	Unit Width:  15 inches (381 mm).

C.	Unit Height:	
1.	75 inches (1,905 mm) with base.
2.	72 inches (1,828 mm) without base.
	D.	Unit Depth:  18 inches (457 mm).

	E.	Unit Assembly:
		1.	One-wide units come fully assembled.
		2.	Three-wide units require minor assembly.

F.	Unit Color:
		1.	Color: Gray - standard.
		2.	Color: Tan - standard.
		3.	Color: Blue - standard.

2.2	INTERIOR EQUIPMENT

B.	Standard Hardware Features: 
	1.	Stainless steel padlock hasp.
		2.	One 10 inch (254 mm) deep shelf (single-tier units only).
		3.	One double prong ceiling hook (single-tier and double-tier units only)
and three single wall hooks (triple-tier units only).
		4.	Horizontal venting.
		5.	Stainless steel door hinges.

2.3	OPTIONAL EQUIPMENT

	A.	Sloping hoods.

B.	Fillers:
	1.	Flat top fillers:
		a.	Flat top in-line top fillers.
		b.	Flat top corner fillers.
	2.	Sloping hood fillers:
		a.	Sloping in-line top fillers.
		b.	Sloping corner fillers.
	3.	Front fillers:
		a.	15 inches (381 mm) wide filler panels.
b.	Vertical corner fillers.

C.	Finished end panels:
	1.	Sloping single end panel, for use with sloping hoods, for end of unit rows.
	2.	Non-sloping single end panel for end of unit rows.

D.	Padlocks:
	1.	Combination padlocks.
	2.	Keyed padlocks.

E.	Master keys:  Master control key for combination padlocks.

F.	Engraved name/number plates.

2.4	CONSTRUCTION
A.	Locker Doors:  Constructed of high density polyethylene (HDPE) with homogeneous color and a matte finish texture.
	1.	Door:
		a.	1/2 inch (12.7 mm) thick HPDE.
		b.	Holes provided for attaching number plates.
	2.	Ventilation:  Ventilation slots provided in standard pattern.
		a.	Single-tier and double-tier lockers:							Four 5-3/4 inch (146 mm) louvers top and bottom
		b.	Triple-tier lockers:
			Three 5-3/4 inch (146 mm) louvers top and bottom.
		c.	Four-tier lockers:
			Two 5-3/4 inch (146 mm) louvers top and bottom.
3.	Latch Bar:  Full-length latch bar is constructed of 1/2 inch (12.7 mm) thick HDPE with a smooth finish; runs entire length of door to provide a continuous security latching system.  Latch bar is secured to door with stainless steel security torx-head shoulder screws.
B.	Locker Body:  Constructed of HDPE.  Frames are welded to locker box to provide a secure, rigid assembly.
C.	Hinges:  Heavy duty full-length piano hinge constructed of 18 gauge stainless steel.  Hinge is secured with stainless steel security torx-head screws and powder coated to match locker finish. 
2.5	MATERIALS
A.	High Density Polyethylene (HDPE):  30 percent pre-consumer recycled content polyethylene thermoplastic formed under high pressure into solid plastic components.
B.	Stainless-Steel Sheet:  ASTM A 666, Type 304.
	C.	Fasteners: Tamper-Resistant Fasteners:  Stainless steel torx-head screws.
		1.	Locker Connectors:  No. 10-24 sex bolt.
2.	Anchors:  Type and size required for secure anchorage.
3.	Drilled-in-place Masonry Anchors: Minimum 1/4 by 1-3/4 inch (6 by 44 mm) screws.

2.6	LOCKER FABRICATION
A.	Fabricate locker box from a single sheet of HDPE solid plastic with corners fused together.  Weld frames and shelves to box assembly.  Provide all welded construction of locker parts without dovetail slots or metal fasteners.  Add welded gussets in single tier full height lockers.
B.	Center Dividers:  Full-depth, vertical partitions between bottom and shelf; finished to match lockers.
C.	Hardware Attachment:  All hinges, handles, hasps, hooks, latch bars, and locks attached with tamper-resistant screws.
D.	Provide ventilated panels where indicated.
E.	Continuous Base:  Set toe clearance 3 inch (76 mm) from locker front.  Notch end caps for ease of installation.
F.	Continuous Sloping Tops:  Fabricated in lengths indicated, without visible fasteners at splice locations; and finished to match lockers.
G.	Filler Panels:  Fabricated in unequal leg angle shape; finished to match lockers.
H.	Finished End Panels:  Fabricated with [3/8 inch (10 mm)] [1/2 inch (13 mm)] wide edge dimension, configured to  conceal fasteners and holes at exposed ends of plastic lockers.

PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding. 

3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.

3.3	INSTALLATION
A.	Install in accordance with Salsbury Industries’ installation instructions.
B.	Anchor the units to the wall studs through the locker back and to the floor.

3.4	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION